GSIC - Global Service Information Center

# VACUUM SWITCHING VALVE (for Unleaded Gasoline Specification Vehicle) > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE VACUUM SWITCHING VALVE (for EVAP)

1. Disconnect the VSV connector.

1. Disconnect the 2 hoses from the VSV.

1. Remove the bolt and VSV.