GSIC - Global Service Information Center

### COMMON RAIL > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE UNDER COVER (for 4WD)

3. REMOVE NO. 2 ENGINE UNDER COVER (for 4WD)

4. DRAIN ENGINE OIL

5. LOOSEN FUEL TANK CAP ASSEMBLY

6. DRAIN FUEL

7. REMOVE NO. 1 ENGINE COVER SUB-ASSEMBLY

8. REMOVE CHARGE AIR COOLER ASSEMBLY WITH INTAKE AIR CONNECTOR

9. REMOVE MANIFOLD STAY

10. REMOVE OIL FILTER SUB-ASSEMBLY

11. REMOVE INJECTION PIPE

12. REMOVE NO. 2 NOZZLE LEAKAGE PIPE ASSEMBLY

13. REMOVE FUEL INLET PIPE SUB-ASSEMBLY

14. REMOVE COMMON RAIL ASSEMBLY