GSIC - Global Service Information Center

# GENERATOR > INSTALLATION

## for Preparation Click here

1. INSTALL GENERATOR ASSEMBLY

1. Install the generator and adjusting bar with the 2 bolts.

   Torque:
     43 N*m{ 438 kgf*cm , 32 ft.*lbf }

1. Install the generator wire with the nut.

   Torque:
     9.8 N*m{ 100 kgf*cm , 87 in.*lbf }

1. Connect the generator connector.

2. INSTALL DRIVE BELT

3. INSTALL V-BANK COVER

1. While turning the belt tensioner counterclockwise, align its holes, and then insert a bar of 6 mm (0.24 in.) into the holes to fix the belt tensioner.

1. Install the V-ribbed belt.

1. While turning the belt tensioner counterclockwise, remove the bar.

1. If it is hard to install the V-ribbed belt, perform the following procedure.

   1. Put the V-ribbed belt on everything except the P/S pump as shown in the illustration.

   2. While releasing the belt tension by turning the belt tensioner counterclockwise, put the V-ribbed belt on the P/S pump.

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.