GSIC - Global Service Information Center

# VALVE BODY > REASSEMBLY

## for Preparation Click here

1. INSTALL SHIFT SOLENOID VALVE S2

1. Install the O-ring to the shift solenoid valve S2.

1. Install the bolt and shift solenoid valve S2.

   Torque:
     10 N*m{ 102 kgf*cm , 7 ft.*lbf }

2. INSTALL SHIFT SOLENOID VALVE S1

1. Install the O-ring to the shift solenoid valve S1.

1. Install the bolt and shift solenoid valve S1.

   Torque:
     6.4 N*m{ 65 kgf*cm , 57 in.*lbf }

3. INSTALL SHIFT SOLENOID VALVE SL1

1. Install the shift solenoid valve SL1.

4. INSTALL SHIFT SOLENOID VALVE SLT

1. Install the shift solenoid valve SLT.

1. Install the bolt, 2 straight pins and solenoid lock plate.

   Torque:
     6.4 N*m{ 65 kgf*cm , 57 in.*lbf }

5. INSTALL SHIFT SOLENOID VALVE SL2

1. Install the shift solenoid valve SL2.

6. INSTALL SHIFT SOLENOID VALVE SLU

1. Install the shift solenoid valve SLU.

1. Install the bolt, 2 straight pins and solenoid lock plate.

   Torque:
     6.4 N*m{ 65 kgf*cm , 57 in.*lbf }

7. INSTALL SHIFT SOLENOID VALVE SR

1. Install the 2 bolts and shift solenoid valve SR.

   Torque:
     6.4 N*m{ 65 kgf*cm , 57 in.*lbf }

8. INSTALL TRANSMISSION VALVE BODY ASSEMBLY

1. Align the groove of the manual valve with the pin of the lever.

1. Install the 19 bolts.

   Torque:
     11 N*m{ 110 kgf*cm , 8 ft.*lbf }

   HINT:
     Bolt length:
     25 mm (0.98 in.) for bolt A
     36 mm (1.42 in.) for bolt B