GSIC - Global Service Information Center

# ROOF HEADLINING (for Extra Cab) > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE FRONT DOOR SCUFF PLATE LH

1. Using a screwdriver, detach the 8 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 4 clips and remove the scuff plate.

3. REMOVE FRONT DOOR SCUFF PLATE RH

HINT:

  Use the same procedures described for the LH side.

4. REMOVE FRONT DOOR OPENING TRIM LH

5. REMOVE FRONT DOOR OPENING TRIM RH

6. REMOVE COWL SIDE TRIM BOARD LH

1. Remove the cap nut.

1. Using a clip remover, detach the 2 clips and remove the trim board.

7. REMOVE COWL SIDE TRIM BOARD RH

HINT:

  Use the same procedures described for the LH side.

8. REMOVE FRONT PILLAR GARNISH LH

1. w/ Assist grip:
   Using a screwdriver, detach the 4 claws and pry out the 2 assist grip plugs.

   HINT:
     Tape the screwdriver tip before use.

1. w/ Assist grip:
   Remove the 2 screws and the assist grip.

1. Using a clip remover, detach the 2 clips.

1. Pull the garnish in the direction indicated by the arrow in the illustration to detach the 2 claws. Then remove the garnish.

9. REMOVE FRONT PILLAR GARNISH RH

HINT:

  Use the same procedures described for the LH side.

10. REMOVE BACK PANEL GARNISH UPPER

1. Using a screwdriver, detach the 4 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 5 clips and remove the garnish.

11. REMOVE REAR SEAT CUSHION ASSEMBLY LH

1. Pull the seat cushion lock hook's release lever in the direction of the arrow, and then disconnect the hook on the front of the seat cushion.

1. Detach the seat cushion's 2 rear hooks from the vehicle body.

1. Remove the seat cushion.

12. REMOVE REAR SEAT CUSHION ASSEMBLY RH

HINT:

  Use the same procedures described for the LH side.

13. REMOVE BACK PANEL GARNISH LOWER

1. Using a screwdriver, detach the 6 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 5 clips and remove the garnish.

14. REMOVE REAR SEATBACK ASSEMBLY

1. Remove the 2 bolts.

1. Lift up the seatback in the direction indicated by the arrow in the illustration to detach the 2 hooks from the vehicle body. Then remove the seatback.

   NOTICE:
     Be careful not to damage the vehicle body.

15. REMOVE FRONT SEAT OUTER BELT ASSEMBLY LH

1. Single cab:
   Remove the outer belt shoulder anchor.

   1. Using a screwdriver, detach the 2 claws and open the seat belt anchor cover.

      HINT:
        Tape the screwdriver tip before use.

   2. Remove the bolt and shoulder anchor.

1. Double cab:
   Remove the outer belt shoulder anchor.

   1. Using a screwdriver, disengage the 4 claws and remove the seat belt anchor cover cap.

      HINT:
        Tape the screwdriver tip before use.

   2. Remove the bolt and shoulder anchor.

1. w/o Pretensioner:
   Remove the bolt and seat belt.

1. w/ Pretensioner:

   1. Disconnect the pretensioner connector as shown in the illustration.

   2. Remove the bolt and seat belt.

16. REMOVE FRONT SEAT OUTER BELT ASSEMBLY RH

1. Single cab:
   Remove the outer belt shoulder anchor.

   1. Using a screwdriver, detach the 2 claws and open the seat belt anchor cover.

      HINT:
        Tape the screwdriver tip before use.

   2. Remove the bolt and shoulder anchor.

1. Double cab:
   Remove the outer belt shoulder anchor.

   1. Using a screwdriver, disengage the 4 claws and remove the seat belt anchor cover cap.

      HINT:
        Tape the screwdriver tip before use.

   2. Remove the bolt and shoulder anchor.

1. w/o Pretensioner:
   Remove the bolt and seat belt.

1. w/ Pretensioner:

   1. Disconnect the pretensioner connector as shown in the illustration.

   2. Remove the bolt and seat belt.

17. REMOVE REAR NO. 1 SEAT BELT ASSEMBLY OUTER LH

1. Remove the bolt and floor anchor.

1. Using a screwdriver, detach the 2 claws and open the seat belt anchor cover.

   HINT:
     Tape the screwdriver tip before use.

1. Remove the bolt.

1. Remove the bolt and seat belt.

18. REMOVE REAR NO. 1 SEAT BELT ASSEMBLY OUTER RH

1. Remove the bolt and floor anchor.

1. Using a screwdriver, detach the 2 claws and open the seat belt anchor cover.

   HINT:
     Tape the screwdriver tip before use.

1. Remove the bolt.

1. Remove the bolt and seat belt.

19. REMOVE QUARTER INSIDE TRIM BOARD LH

1. Using a clip remover, detach the 7 clips.

1. Using a screwdriver, detach the 6 claws and remove the trim board.

   HINT:
     Tape the screwdriver tip before use.

1. Detach the claws and remove the trim pocket from the trim board.

20. REMOVE QUARTER INSIDE TRIM BOARD RH

HINT:

  Use the same procedures described for the LH side.

21. REMOVE QUARTER PILLAR GARNISH LH

1. Using a clip remover, detach the 2 clips and remove the garnish.

22. REMOVE QUARTER PILLAR GARNISH RH

HINT:

  Use the same procedures described for the LH side.

23. REMOVE ROOF SIDE GARNISH INNER UPPER LH

1. Using a clip remover, detach the 3 clips and remove the garnish.

24. REMOVE ROOF SIDE GARNISH INNER UPPER RH

HINT:

  Use the same procedures described for the LH side.

25. REMOVE ROOM LIGHT ASSEMBLY

Click here

26. REMOVE VISOR ASSEMBLY LH

1. Remove the 2 screws and visor.

27. REMOVE VISOR ASSEMBLY RH

1. Remove the 2 screws and visor.

28. REMOVE VISOR HOLDER LH

1. Remove the screw.

1. Using a screwdriver, detach the 2 claws and remove the holder.

   HINT:
     Tape the screwdriver tip before use.

29. REMOVE VISOR HOLDER RH

HINT:

  Use the same procedures described for the LH side.

30. REMOVE ASSIST GRIP

1. Using a screwdriver, detach the 4 claws and open the 2 covers.

   HINT:
     Tape the screwdriver tip before use.

1. Remove the 2 screws and assist grip.

31. REMOVE ROOF HEADLINING ASSEMBLY

1. Using a clip remover, remove the 5 clips and headlining.

1. Remove the wire harness.

32. REMOVE ROOF NO. 2 SILENCER PAD

33. REMOVE SIDE RAIL SPACER FRONT LH

34. REMOVE SIDE RAIL SPACER FRONT RH

35. REMOVE SIDE RAIL SPACER REAR LH (for LHD)

36. REMOVE SIDE RAIL SPACER REAR RH (for RHD)

37. REMOVE NO. 2 SIDE RAIL SPACER REAR LH

38. REMOVE NO. 2 SIDE RAIL SPACER REAR RH

39. REMOVE NO. 3 SIDE RAIL SPACER REAR LH

40. REMOVE NO. 3 SIDE RAIL SPACER REAR RH