GSIC - Global Service Information Center

### DTC 61-40 Mechanical Error of Media (AUDIO H/U)

## for Preparation Click here

## DESCRIPTION

DTC No. | DTC Detection Condition | Trouble Area

61-40

Malfunction due to mechanical failure is identified, or cassette tape is cut or entangled.

1. Cassette tape
2. Radio receiver assembly

## INSPECTION PROCEDURE

1.PRESS ''EJECT'' AND CHECK OPERATION

1. Press the cassette tape EJECT switch of the radio receiver for 2 seconds or more and check that the cassette tape is ejected.

   OK:
     Cassette tape is ejected.

| NG |

REPLACE RADIO RECEIVER ASSEMBLY

OK |

2.CHECK CASSETTE TAPE

1. Check that the ejected cassette tape does not have a peeling label, cassette body deformation or other problems.

   OK:
     No problem with cassette tape.

| NG |

CASSETTE TAPE IS FAULTY

OK |

3.REPLACE CASSETTE TAPE WITH ANOTHER AND RECHECK

1. Replace the cassette tape with a normal one and check if the same problem occurs again.

   OK:
     Malfunction disappears.

| NG |

REPLACE RADIO RECEIVER ASSEMBLY

OK |

CASSETTE TAPE IS FAULTY