GSIC - Global Service Information Center

# FRONT SEAT ASSEMBLY (for Separate Seat Type) > INSTALLATION

## for Preparation Click here

1. INSTALL FRONT SEAT ASSEMBLY

1. Place the seat in the cabin.

   NOTICE:
     Be careful not to damage the vehicle body.

1. w/ Seat belt warning, w/ occupant detection sensor:
   Connect the connector under the seat.

1. Install the seat with the 4 bolts.

   Torque:
     37 N*m{ 377 kgf*cm , 27 ft.*lbf }

   HINT:
     Tighten the bolts in the order indicated in the illustration.

2. INSPECT AND ADJUST SEAT SLIDE ADJUSTER LOCKS

1. During sliding operation of the front seat, check that the left and right adjusters move together smoothly and lock simultaneously.
   If the seat adjusters do not lock simultaneously, loosen the seat fixation bolts to adjust the adjuster's position.

3. INSTALL FRONT SEAT HEADREST ASSEMBLY

4. INSTALL SEAT TRACK BRACKET COVER INNER RH (Except Single Cab)

1. Install the bracket cover in the direction indicated by the arrow in the illustration and attach the 2 claws.

5. INSTALL SEAT TRACK BRACKET COVER OUTER RH (Except Single Cab)

1. Install the bracket cover in the direction indicated by the arrow in the illustration and attach the 2 claws.

6. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

7. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.