GSIC - Global Service Information Center

# FRONT WIPER RUBBER > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the RH side and LH side.
2. The procedures listed below are for the LH side.

1. REMOVE FRONT WIPER BLADE

1. Detach the claw as shown in the illustration.

1. Remove the wiper blade as shown in the illustration.

   NOTICE:
     Do not fold the wiper arm with the wiper blade removed. The arm tip may damage the windshield surface.

2. REMOVE WIPER RUBBER

1. Detach the head part (large side) of the wiper rubber from the wiper blade.

1. Remove the wiper rubber in the direction indicated by the arrow in the illustration.

   NOTICE:
     Do not pull out the wiper rubber forcibly. Doing so will deform the backing plate or damage the blade claw.

1. Remove the 2 wiper rubber backing plates from the wiper rubber.