GSIC - Global Service Information Center

# FUEL PRESSURE PULSATION DAMPER > INSTALLATION

## for Preparation Click here

1. INSTALL FUEL PRESSURE PULSATION DAMPER ASSEMBLY

1. Apply a light coat of spindle oil or gasoline to a new O-ring and install it to the fuel pressure pulsation damper.

1. Install the fuel pressure pulsation damper to the fuel delivery pipe.

1. Install the clip.

2. INSTALL INTAKE AIR SURGE TANK

1. Install a new gasket and the surge tank with the 2 nuts.

   Torque:
     28 N*m{ 286 kgf*cm , 21 ft.*lbf }

1. Using an 8 hexagon wrench, install the 4 bolts.

   Torque:
     28 N*m{ 286 kgf*cm , 21 ft.*lbf }

1. Install the 3 upper bolts which are used to secure the 2 surge tank stays and throttle body bracket.

   Torque:
     21 N*m{ 214 kgf*cm , 16 ft.*lbf }

1. Install the 3 wire harness clamps and hose clamp.

1. Connect the throttle motor connector.

1. Connect the 2 VSV connectors.

1. Connect the ventilation hose.

1. Connect the vapor feed hose assembly.

1. Connect the No. 4 water by-pass hose.

1. Connect the No. 5 water by-pass hose.

3. INSTALL AIR CLEANER ASSEMBLY

Torque:
  8.0 N*m{ 82 kgf*cm , 71 in.*lbf }

4. CONNECT NO. 2 VENTILATION HOSE

5. INSTALL V-BANK COVER

1. Install the cover with the 2 nuts.

   Torque:
     7.5 N*m{ 76.5 kgf*cm , 66 in.*lbf }

6. CONNECT CABLE TO BATTERY NEGATIVE TERMINAL

7. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

8. CHECK FOR FUEL LEAKS

1. Connect the intelligent tester to the DLC3.

   1. Turn the ignition switch ON.

      NOTICE:
        Do not start the engine.

   2. Push the intelligent tester main switch ON.

   3. Select Active Test and enter the following menus: Powertrain / Engine and ECT / Active Test / Control the Fuel Pump / Speed.

1. Check for fuel leaks.

   1. Check that there are no fuel leaks after performing maintenance anywhere on the fuel system.