GSIC - Global Service Information Center

# EXHAUST PIPE > REMOVAL

## for Preparation Click here

CAUTION:

1. Wear protective gloves when removing the exhaust pipe.

1. The exhaust pipe is extremely hot immediately after the engine has stopped.

1. Confirm that the exhaust pipe has cooled down before removing it.

1. REMOVE TAILPIPE ASSEMBLY

1. Remove the 2 bolts and 2 nuts.

1. Disconnect the tailpipe from the center pipe and remove the gasket.

1. Remove the tailpipe from the pipe support.

2. REMOVE CENTER EXHAUST PIPE ASSEMBLY

1. Remove the 2 bolts and 2 nuts.

1. Disconnect the center pipe from the front pipe and remove the gasket.

1. Remove the center pipe from the 3 pipe supports.

3. REMOVE FRONT EXHAUST PIPE ASSEMBLY

1. Remove the 2 bolts and 2 compression springs.

1. Disconnect the front pipe from the outlet pipe and remove the gasket.

1. Remove the front pipe from the pipe support.