GSIC - Global Service Information Center

# EMISSION CONTROL SYSTEM (for Leaded Gasoline Specification Vehicle) > ON-VEHICLE INSPECTION

## for Preparation Click here

1. VISUALLY CHECK HOSES, CONNECTIONS AND GASKETS

1. Check that there are no cracks, leaks or damage.

   NOTICE:
   1. Detachment or other problems with the engine oil dipstick, filler cap, PCV hose and other components may cause the engine to run improperly.
   1. Air suction caused by disconnections, looseness or cracks in the parts of the air induction system between the throttle body and cylinder head will cause engine failure or engine malfunctions.
   If the result is not as specified, replace parts as necessary.