GSIC - Global Service Information Center

# REAR SEAT INNER BELT ASSEMBLY > REMOVAL

## for Preparation Click here

HINT:

  A bolt without a torque specification is shown in the standard bolt chart (Click here ).

1. REMOVE REAR SEAT ASSEMBLY (for Double Cab)

1. Using a screwdriver, detach the 2 claws labeled A.

   HINT:
     Tape the screwdriver tip before use.

1. Pull the hinge cover in the direction indicated by the arrow in the illustration to detach the claw labeled B. Then remove the hinge cover.

2. REMOVE REAR NO. 1 SEAT BELT ASSEMBLY INNER RH (for Double Cab)

1. Remove the bolt and seat belt.

3. REMOVE REAR NO. 1 SEAT BELT ASSEMBLY INNER LH (for Double Cab)

1. Remove the bolt and seat belt.

4. REMOVE REAR NO. 1 SEAT BELT ASSEMBLY INNER (for Extra Cab)

1. Remove the bolt and seat belt.