GSIC - Global Service Information Center

# FLOOR SHIFT ASSEMBLY > ADJUSTMENT

## for Preparation Click here

1. INSPECT SHIFT LEVER POSITION

1. When moving the shift lever from P to R with the ignition switch ON and the brake pedal depressed, make sure that the shift lever moves smoothly and correctly into position.

1. Start the engine and make sure that the vehicle moves forward after moving the shift lever from N to D, and moves rearward after shifting to the.
   If the results are not as specified, inspect the park/neutral position switch and check the shift lever.

2. ADJUST SHIFT LEVER POSITION

1. Remove the nut and disconnect the control cable.

1. Remove the clip and disconnect the control cable from the control cable bracket.

1. Push the control shaft rearward as much as possible.

1. Return the control shaft lever 2 notches to the N position.

1. While holding the control shaft lever slightly toward the R position side, tighten the nut.

   Torque:
     15.6 N*m{ 159 kgf*cm , 12 ft.*lbf }