GSIC - Global Service Information Center

# SPEED SENSOR > INSPECTION

## for Preparation Click here

1. INSPECT TRANSMISSION REVOLUTION SENSOR (NT)

1. Measure the resistance of the sensor.

   Standard resistance:

     Tester Connection | Condition | Specified Condition
     1 - 2 | 20°C (68°F) | 560 to 680 Ω

2. INSPECT VEHICLE SPEED SENSOR (SP2)

1. Measure the resistance of the sensor.

   Standard resistance:

     Tester Connection | Condition | Specified Condition
     1 - 2 | 20°C (68°F) | 560 to 680 Ω