GSIC - Global Service Information Center

# 1KD-FTV INTAKE > SERVICE DATA

Intake manifold (swirl control valve):

  Engine Condition | VSV Condition | Specified Condition
  Normal engine speed | ON | Approximately 35 kPa (263 mmHg, 10.35 in.Hg)
  3,000 rpm or more | OFF | 0 kPs (0 mmHg, 0 in.Hg)

Vacuum switching valve (for swirl control valve):

  Tester Connection | Specified Condition
  1 - 2 | 33 to 39 Ω at 20°C (68°F)
  1 - Body ground 2 - Body ground | 1 MΩ or higher

Turbocharger pressure:

  Condition | Specified Condition
  Engine speed (approximately 4,600 rpm) | 15 to 45 kPs (0.15 to 0.46 kgf*cm2, 2.1 to 6.5 psi)

Manifold absolute pressure sensor:

  Condition | Tester Connection | Specified Condition
  ECM output voltage | T9-3 (VC (+)) - T9-1 (E2 (-)) | 4.5 to 5.5 V
  Applied vacuum | - | -
  -13.3 kPs (100 mmHg, 3.94 in.Hg) | E7-28 (PIM) - E8-28 (E2) | 0.1 to 0.4 V
  -26.6 kPs (199 mmHg, 7.85 in.Hg) | 0.2 to 0.6 V
  -40 kPs (300 mmHg, 11.81 in.Hg) | 0.4 to 0.8 V
  Applied pressure | - | -
  19.6 kPs (0.20 mmHg, 2.84 in.Hg) | E7-28 (PIM) - E8-28 (E2) | 0.1 to 0.4 V
  39.2 kPs (0.40 mmHg, 5.69 in.Hg) | 0.4 to 0.7 V
  58.8 kPs (0.60 mmHg, 8.53 in.Hg) | 0.7 to 1.0 V
  78.5 kPs (0.80 mmHg, 11.4 in.Hg) | 1.0 to 1.3 V
  98.0 kPs (1.00 mmHg, 14.2 in.Hg) | 1.3 to 1.6 V

Turbocharger:

  Condition | Specified Condition
  Maximum axial play of turbine shaft | 0.11 mm (0.0043 in.)
  Maximum radial play of turbine shaft | 0.112 mm (0.0044 in.)