GSIC - Global Service Information Center

# IGNITION SWITCH > INSTALLATION

## for Preparation Click here

1. INSTALL IGNITION OR STARTER SWITCH ASSEMBLY

1. Install the switch to the steering column bracket upper with the 2 claws.

2. CONNECT CONNECTOR

1. Connect the 9 connectors as shown in the illustration.

1. Secure the wire harness with the clamps.

3. INSTALL STEERING COLUMN COVER LOWER

1. Install the cover lower with the 3 screws.

   HINT:
     Turn the steering wheel to the right and left as necessary to install the 3 screws and cover lower.

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

Perform initialization (Click here).

NOTICE:

  Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.