GSIC - Global Service Information Center

# LOAD SENSING PROPORTIONING VALVE > DISASSEMBLY

## for Preparation Click here

1. REMOVE REAR FLEXIBLE HOSE BRACKET

1. Remove the 2 nuts.

1. Remove the bracket and valve set plate from the valve.

2. REMOVE LOAD SENSING VALVE BRACKET

1. Remove the bolt, nut and 2 washers.

1. Remove the bracket from the valve.

3. REMOVE LOAD SENSING SPRING ASSEMBLY

1. Using pliers, remove the clip and spring from the valve body.

4. REMOVE NO. 1 AND NO. 2 SHACKLES

1. Remove the bolt, nut and 2 plate washers.

1. Remove the No. 1 shackle (with No. 2 shackle) from the spring.

1. Loosen the lock nut.

1. Remove the adjusting nut and No. 2 shackle from the No. 1 shackle.

5. REMOVE LOAD SENSING SPRING

1. Remove the 4 bushes, 2 collars and 2 rubber plates from the spring.

1. Remove the valve boot and spring boot from the spring.