GSIC - Global Service Information Center

# OUTER REAR VIEW MIRROR > INSTALLATION

## for Preparation Click here

1. INSTALL OUTER MIRROR COVER LH (w/ Outer mirror cover)

1. Install the mirror cover as shown in the illustration.

1. After installing the outer mirror cover, check that there is no gap between the cover and mirror body.

   HINT:
     If there is a gap between the cover and body, noise will occur during driving.

1. Install the mirror as shown in the illustration.

2. INSTALL OUTER REAR VIEW MIRROR ASSEMBLY LH

1. Install the mirror with the 3 nuts.

   Torque:
     8.0 N*m{ 82 kgf*cm , 71 ft.*lbf }

1. w/ Power mirror control:
   Connect the connector labeled A.

3. INSTALL FRONT DOOR TRIM BOARD SUB-ASSEMBLY LH

1. Install the frame with the 2 bolts.

   Torque:
     8.0 N*m{ 82 kgf*cm , 71 in.*lbf }

4. INSTALL FRONT DOOR LOWER FRAME BRACKET GARNISH LH (w/ Power Mirror control)

1. Attach the 2 clips to install the garnish.

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.