GSIC - Global Service Information Center

# 2TR-FE LUBRICATION > TORQUE SPECIFICATIONS

Part tightened | N*m | kgf*cm | ft.*lbf
Oil pressure switch x Cylinder block | 15 | 153 | 11
Oil filter x Oil filter union | 17.2 | 175 | 13
Oil drain plug x No. 2 oil pan | 37.5 | 382 | 28
Oil pump cover x Timing chain cover | 9.0 | 92 | 80 in.*lbf
Oil pump relief valve x Timing chain cover | 49 | 500 | 36
Water pump x Timing chain cover | 9.0 | 92 | 80 in.*lbf
Timing chain cover x Cylinder block : Excluding bolt A, tighten the bolts and nuts in this order: Area 1, Area 2, Area 3 | 21 | 214 | 15
Timing chain cover x Cylinder block : Tighten the bolts labeled A in this order: Area 2 and Area 3: | 46 | 469 | 34
Timing chain cover x Cylinder block : Tighten the bolts labeled E for Area 4 | 21 | 214 | 15
No. 1 oil pan x Cylinder block | 26 | 265 | 19
Oil strainer x No. 1 oil pan | 20 | 204 | 15
No 2 oil pan x No. 1 oil pan | 9.0 | 92 | 80 in.*lbf
Crank pulley bolt x Crankshaft | 260 | 2,651 | 192
Camshaft position sensor x Cylinder head | 8.5 | 87 | 75 in.*lbf
Cylinder head cover x Cylinder head | 9.0 | 92 | 80 in.*lbf
No. 1 water by-pass pipe x Timing chain cover | 17.5 | 179 | 13
No. 1 idler pulley x Timing chain cover | 43 | 438 | 32
V-ribbed belt tensioner x Timing chain cover : for bolt 1 | 40 | 408 | 30
V-ribbed belt tensioner x Timing chain cover : for bolt 2 | 21 | 214 | 15
V-ribbed belt tensioner x Timing chain cover : for bolt 3 | 43 | 438 | 32
Intake manifold x Cylinder head | 25 | 255 | 18