GSIC - Global Service Information Center

# 1KD-FTV INTAKE > TORQUE SPECIFICATIONS

Intake manifold:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Intake manifold x Cylinder head | 29 | 296 | 21
  Oil level gauge guide x Intake manifold | 8.0 | 82 | 71 in.*lbf
  Oil level gauge guide x Injection pipe clamp | 5.0 | 51 | 44 in.*lbf
  Manifold stay x Intake manifold | 19 | 194 | 14
  Manifold stay x Cylinder head
  No. 1 EGR pipe sub-assembly x EGR valve | 19 | 194 | 14
  No. 1 EGR pipe sub-assembly x Cylinder head
  Intake air connector x Intake manifold | 20 | 204 | 15
  Throttle body bracket x Intake manifold, intake air connector | 20 | 204 | 15
  Throttle body bracket x Intake air connector
  Vacuum switching valve bracket x Intake air connector | 20 | 204 | 15
  Vacuum switching valve bracket x Intake manifold

Turbocharger:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Turbocharger x Exhaust manifold | 52 | 530 | 38
  Turbo oil inlet pipe sub-assembly x Turbocharger | 13 | 133 | 10
  Turbo oil inlet pipe sub-assembly x Cylinder block | Bolt | 12 | 122 | 9
  Union bolt | 26 | 265 | 19
  Turbocharger stay x Turbocharger | 24 | 245 | 18
  Turbocharger stay x Cylinder block
  Turbine outlet elbow x Turbocharger | 26 | 265 | 19
  Exhaust manifold heat insulator x Exhaust manifold | 12 | 122 | 9
  No. 1 turbo insulator x Turbocharger | 12 | 122 | 9
  Compressor inlet elbow x Turbocharger | 19 | 194 | 14
  Ventilation hose x Cylinder head cover | 20 | 204 | 15
  Air cleaner assembly x Body panel | 14 | 143 | 10

Intercooler:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Intake air connector x Charge air cooler | 10 | 102 | 7
  IAT sensor x Charge air cooler | 29.4 | 300 | 22
  Charge air cooler x Stay | 12 | 122 | 9
  Charge air cooler x Intake manifold | 32 | 326 | 24
  No. 1 air hose x Diesel throttle body assembly | 6.5 | 66 | 58 in.*lbf
  No. 2 air hose x Turbocharger | 6.5 | 66 | 58 in.*lbf
  Manifold absolute pressure sensor x Charge air cooler | 6.0 | 61 | 53 in.*lbf
  No. 1 gas filter x Charge air cooler | 6.0 | 61 | 53 in.*lbf
  No. 1 engine cover sub-assembly x Stay | 7.0 | 71 | 62 in.*lbf