GSIC - Global Service Information Center

# 2KD-FTV COOLING > TORQUE SPECIFICATIONS

Coolant:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Cylinder block drain cock plug x Oil cooler cover sub-assembly | 8.0 | 82 | 71 in.*lbf
  Vent plug x Radiator tank upper | 2.0 | 20 | 18 in.*lbf

Water pump:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Water pump assembly x Cylinder block | 13 | 133 | 10
  V-ribbed belt tensioner assembly x Cylinder block | 21 | 214 | 15
  V-ribbed belt tensioner assembly x Water pump assembly
  Cooler compressor assembly x engine | 24.5 | 250 | 18
  Fan shroud x Radiator tank upper | 5.0 | 51 | 44 in.*lbf
  Fluid coupling fan x Water pump assembly | 18 | 184 | 13
  Radiator reservoir x Radiator tank upper | 5.0 | 51 | 44 in.*lbf
  Oil reservoir x Radiator tank upper | 5.0 | 51 | 44 in.*lbf
  No. 1 engine under cover x Body | 28 | 286 | 21

Thermostat:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Water inlet x Cylinder block | 13 | 133 | 10

Fan:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Fan x Fluid coupling | 6.0 | 61 | 53 in.*lbf
  No. 1 engine under cover x Body | 28 | 286 | 21

Radiator:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Radiator assembly x Body panel | 12 | 122 | 9
  No. 1 engine under cover x Body | 28 | 286 | 21