GSIC - Global Service Information Center

# 1GR-FE LUBRICATION > SERVICE DATA

Oil pressure : at idle | 29 kPa (0.3 kgf/cm2, 4.2 psi) or more
Oil pressure : at 3,000 rpm | 294 to 588 kPa (3.0 to 6.0 kgf/cm2, 4.3 to 85 psi) or more
Oil pump : Tip clearance | Standard: 0.060 to 0.160 mm (0.0016 to 0.0063 in.) Maximum: 0.16 mm (0.0063 in.)
Oil pump : Side clearance | Standard: 0.030 to 0.090 mm (0.0012 to 0.0035 in.) Maximum: 0.090 mm (0.0035 in.)
Oil pump : Body clearance | Standard: 0.250 to 0.325 mm (0.0098 to 0.0128 in.) Maximum: 0.325 mm (0.0128 in.)