GSIC - Global Service Information Center

# VENTILATION VALVE > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE V-BANK COVER

1. Remove the 2 nuts and cover.

3. REMOVE INTAKE AIR SURGE TANK

1. Disconnect the No. 5 water by-pass hose.

1. Disconnect the No. 4 water by-pass hose.

1. Disconnect the fuel vapor feed hose assembly.

1. Disconnect the ventilation hose.

1. Disconnect the 2 VSV connectors.

1. Disconnect the throttle motor connector.

1. Remove the 3 wire harness clamps and hose clamp.

1. Remove the 3 upper bolts, which are used to secure the 2 surge tank stays and throttle body bracket.

1. Using an 8 mm hexagon wrench, remove the 4 bolts.

1. Remove the 2 nuts, intake air surge tank and gasket.

4. REMOVE VENTILATION VALVE SUB-ASSEMBLY

1. Loosen the hose clamp and disconnect the ventilation hose from the valve.

1. Remove the valve.