GSIC - Global Service Information Center

# SEAT > TORQUE SPECIFICATIONS

FRONT SEAT (FOR SEPARATE SEAT TYPE):

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Seatback spring x Seat cushion frame | 40 | 408 | 30
  Front seat inner belt x Seat cushion | 42 | 428 | 31
  Seat cushion frame x Reclining adjuster arm | 19.5 | 199 | 14
  Seat adjuster rod x Reclining adjuster arm w/ Vertical adjuster | 19.5 | 199 | 14
  Reclining adjuster arm x Seat track w/ Vertical adjuster | 25 | 255 | 18
  Reclining adjuster arm x Seat track w/o Vertical adjuster | 19.5 | 199 | 14
  Front seat x Body | 37 | 377 | 27

FRONT SEAT (FOR BENCH SEAT TYPE):

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Seatback spring x Seat cushion frame | 40 | 408 | 30
  Front seat x Body | 37 | 377 | 27

REAR SEAT (FOR DOUBLE CAB):

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Seatback frame x Seat cushion frame | 19.5 | 199 | 199
  Seat leg bracket x Seat cushion frame | 14.5 | 148 | 11
  Front seat x Body | 19.5 | 199 | 199

REAR SEAT (FOR EXTRA CAB):

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Seatback x Body | 39 | 398 | 29