GSIC - Global Service Information Center

### AIRBAG SYSTEM > SRS Warning Light Remains ON

## for Preparation Click here

## DESCRIPTION

The SRS warning light is located on the combination meter. When the SRS is normal, the SRS warning light illuminates for approximately 6 seconds after the ignition switch is turned from OFF to ON, and then turns OFF automatically. If there is a malfunction in the SRS, the SRS warning light illuminates to inform the driver. When terminals TC and CG of the DLC3 are connected, the DTCs are communicated through SRS warning light blinking patterns.

## WIRING DIAGRAM

## INSPECTION PROCEDURE

1.INSPECT BATTERY

1. Measure the voltage of the battery.

   Standard voltage:
     11 to 14 V

| NG |

RECHARGE OR REPLACE BATTERY

OK |

2.CHECK CONNECTION OF CONNECTOR

1. Disconnect the cable from the negative (-) battery terminal, and wait for at least 90 seconds.

1. Check that the connector is properly connected to the center airbag sensor.

   OK:
     Connector is connected.

| NG |

CONNECT CONNECTOR

OK |

3.PREPARE FOR INSPECTION

CAUTION:

  Be sure to perform the following procedures before troubleshooting to avoid unexpected airbag deployment.

1. Disconnect the connector from the center airbag sensor.

1. Disconnect the connector from the steering pad connector.

NEXT |

4.CHECK CENTER AIRBAG SENSOR ASSEMBLY

1. Connect the cable to the negative (-) battery terminal, and wait for at least 2 seconds.

1. Turn the ignition switch ON.

1. Measure the voltage and resistance of the wire harness side connector.

   Standard voltage:

     Tester Connection | Specified Condition
     A14-21 (IG2) - Body ground | 8 to 14 V

   Standard resistance:

     Tester Connection | Specified Condition
     A14-25 (E1) - Body ground | Below 1 Ω

| NG |

REPAIR OR REPLACE HARNESS AND CONNECTOR

OK |

5.CHECK COMBINATION METER ASSEMBLY (POWER SOURCE)

1. Disconnect the C8 meter connector.

1. Turn the ignition switch ON.

1. Measure the voltage of the wire harness side connector.

   Standard voltage:

     Tester Connection | Specified Condition
     C8-21 - Body ground | 8 to 14 V

| NG |

REPAIR OR REPLACE HARNESS AND CONNECTOR

OK |

6.CHECK WIRE HARNESS (CENTER AIRBAG SENSOR ASSEMBLY - COMBINATION METER ASSEMBLY AND BODY GROUND)

1. Disconnect the A14 ECU connector.

1. Disconnect the C8 meter connector.

1. Measure the resistance of the wire harness side connectors.

   Standard resistance:

     Tester Connection | Specified Condition
     A14-14 (LA) - C8-20 | Below 1 Ω

| NG |

REPAIR OR REPLACE HARNESS AND CONNECTOR

OK |

7.CHECK SRS WARNING LIGHT OPERATION

1. Disconnect the A14 ECU connector with the C8 meter connector connected.

1. Turn the ignition switch ON.

1. Check that the warning light illuminates 10 seconds after turning the ignition switch ON.

   OK:
     Warning light illuminates 10 seconds after turning ignition switch ON.

| NG |

REPLACE COMBINATION METER ASSEMBLY

OK |

8.CHECK CENTER AIRBAG SENSOR ASSEMBLY

1. Disconnect the A14 ECU connector.

1. Turn the ignition switch ON.

1. Measure the voltage of the wire harness side connector.

   Standard voltage:

     Tester Connection | Specified Condition
     A14-14 (LA) - Body ground | 8 to 14 V

| NG |

REPAIR OR REPLACE HARNESS AND CONNECTOR

OK |

9.REPLACE CENTER AIRBAG SENSOR ASSEMBLY

1. Replace the center airbag sensor.

1. Check that the SRS warning light illuminates normally.

   OK:
     SRS warning light illuminates normally.

| NG |

REPLACE COMBINATION METER ASSEMBLY

OK |

END