GSIC - Global Service Information Center

# TRANSFER ASSEMBLY > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. DRAIN TRANSFER OIL

3. REMOVE LOWER TRANSFER CASE PROTECTOR

1. Remove the 4 bolts and protector.

4. REMOVE MANUAL TRANSMISSION ASSEMBLY (M/T)

1. Remove the manual transmission (Click here).

5. REMOVE AUTOMATIC TRANSMISSION ASSEMBLY (A/T)

1. Remove the automatic transmission (Click here).

6. REMOVE TRANSFER ASSEMBLY

1. Remove the 8 bolts and 2 clamps.

1. Remove the transfer from the transmission.