GSIC - Global Service Information Center

# FRONT PASSENGER AIRBAG ASSEMBLY > INSTALLATION

## for Preparation Click here

CAUTION:

  Be sure to read the precautionary notices concerning the SRS airbag system before servicing (Click here).

1. INSTALL FRONT PASSENGER AIRBAG ASSEMBLY

1. Attach the 12 claws to install the airbag.

1. Attach the clamp to the bracket.

1. Tighten the 2 bolts.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

1. Connect the connector to the airbag.

   NOTICE:
     When handling the airbag connector, do not damage the airbag wire harness.

2. INSTALL GLOVE COMPARTMENT DOOR ASSEMBLY

1. Attach the 2 hinges to install the door.

1. Push in the sides of the glove compartment door, as indicated by the arrows in the illustration. Then close the door to engage it to the 2 stoppers.

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

5. INSPECT SRS WARNING LIGHT

1. Check the SRS warning light (Click here).