GSIC - Global Service Information Center

# FUEL PUMP RESISTOR > INSTALLATION

## for Preparation Click here

1. INSTALL FUEL PUMP RESISTOR

1. Install the resistor with the bolt.

   Torque:
     7.5 N*m{ 76.5 kgf*cm , 66 in.*lbf }

1. Connect the connector.

2. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

3. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.