GSIC - Global Service Information Center

# REAR BRAKE FLEXIBLE HOSE > REMOVAL

## for Preparation Click here

1. DRAIN BRAKE FLUID

NOTICE:

  Wash off brake fluid immediately if it comes in contact with any painted surface.

2. REMOVE REAR BRAKE TUBE FLEXIBLE HOSE

1. Remove the brake tube and 3-way from the flexible hose with SST while holding the flexible hose with a wrench.

   SST
     09023-00101

   NOTICE:
   1. Do not bend or damage the brake tube.
   2. Do not allow any foreign matter such as dirt and dust to enter the brake tube and 3-way from the connecting points.

1. Remove the clip and flexible hose.