GSIC - Global Service Information Center

### DTC 63-48 Excess Current

### DTC 63-51 Elevator Error

### DTC 63-52 Clamp Error

## for Preparation Click here

## DESCRIPTION

DTC No. | DTC Detection Condition | Trouble Area
63-48 | Overcurrent is present in CD changer. | Radio receiver assembly
63-51 | Mechanical error occurred during elevator operation. | Radio receiver assembly
63-52 | Failure in disc clamping or clamp error. | Radio receiver assembly

## INSPECTION PROCEDURE

1.CHECK FOR DTC

1. Delete the DTC.

1. Check for DTCs again.

   OK:
     No DTC is output.

| NG |

REPLACE RADIO RECEIVER ASSEMBLY

OK |

END