GSIC - Global Service Information Center

# VACUUM SWITCHING VALVE > INSTALLATION

## for Preparation Click here

1. INSTALL VACUUM SWITCHING VALVE (for EGR Cut)

1. Install the valve with the bolt.

   Torque:
     3.5 N*m{ 36 kgf*cm , 31 in.*lbf }

2. INSTALL VACUUM SWITCHING VALVE BRACKET

1. Install the bracket with the 2 bolts.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

1. Connect the vacuum hoses to the 3 locations.

1. Connect the 2 connectors.

3. INSTALL CHARGE AIR COOLER ASSEMBLY

1. Install a new gasket and the intake air connector with the 4 bolts.

   Torque:
     10 N*m{ 102 kgf*cm , 7 ft.*lbf }

1. Using a 22 mm deep socket wrench, install a new gasket and the IAT sensor.

   Torque:
     29.4 N*m{ 300 kgf*cm , 22 ft.*lbf }

1. Install the CAC with the 4 bolts.

   Torque:
     32 N*m{ 326 kgf*cm , 24 ft.*lbf } for bolt A

   Torque:
     12 N*m{ 122 kgf*cm , 9 ft.*lbf } for bolt B

1. Tighten the 4 hose clamps of the No. 1 and No. 2 air hose.

   Torque:
     6.5 N*m{ 66 kgf*cm , 58 in.*lbf }

1. Connect the diesel turbo IAT sensor connector.

4. INSTALL NO. 1 ENGINE COVER SUB-ASSEMBLY

1. Install the cover with the 3 bolts and 2 nuts.

   Torque:
     7.0 N*m{ 71 kgf*cm , 62 in.*lbf }

5. CONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

6. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   CAUTION:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from negative (-) battery terminal.