GSIC - Global Service Information Center

# 2KD-FTV INTAKE > SERVICE DATA

Turbocharger pressure:

  Condition | Specified Condition
  Engine speed (approximately 4,600 rpm) | 58.5 to 78.9 kPa 0.60 to 0.80 kgf*cm2, 8.5 to 11.4 psi)

Manifold absolute pressure sensor:

  Condition | Tester connection | Specified Condition
  ECM output voltage | T9-3 (VC (+)) - T9-1 (E2 (-)) | 4.5 to 5.5 V
  Applied vacuum | - | -
  -- 13.3 kPs (100 mmHg, 3.94 in.Hg) | E7-28 (PIM) - E8-28 (E2) | 0.1 to 0.4 V
  -26.6 kPs (199 mmHg, 7.85 in.Hg) | 0.2 to 0.6 V
  -40 kPs (300 mmHg, 11.81 in.Hg) | 0.4 to 0.8 V
  Applied pressure | - | -
  -19. 6 kPs (0.20 mmHg, 2.84 in.Hg) | E7-28 (PIM) - E8-28 (E2) | 0.1 to 0.4 V
  39.2 kPs (0.40 mmHg, 5.69 in.Hg) | 0.4 to 0.7 V
  58.8 kPs (0.60 mmHg, 8.53 in.Hg) | 0.7 to 1.0 V
  78.5 kPs (0.80 mmHg, 11.4 in.Hg) | 1.0 to 1.3 V
  98.0 kPs (1.00 mmHg, 14.2 in.Hg) | 1.3 to 1.6 V

Turbocharger:

  Condition | Specified Condition
  Maximum axial play of turbine shaft | 0.08 mm (0.0031 in.)
  Maximum radial play of turbine shaft | 0.11 mm (0.0043 in.)
  Actuator and waste date valve operation | 144kPa (1.16 kgf*cm2, 16.5 psi)