GSIC - Global Service Information Center

### FRONT BUMPER > REMOVAL

1. REMOVE RADIATOR GRILLE

2. REMOVE FRONT FENDER LINER LH

3. REMOVE ENGINE SIDE COVER SUB-ASSEMBLY LH (for 4WD)

4. REMOVE ENGINE SIDE COVER SUB-ASSEMBLY RH (for 4WD)

5. REMOVE FRONT BUMPER COVER

6. REMOVE FRONT BUMPER SIDE RETAINER LH

7. REMOVE FRONT BUMPER SIDE RETAINER RH

8. REMOVE FRONT BUMPER REINFORCEMENT SUB-ASSEMBLY

9. REMOVE FRONT BUMPER REINFORCEMENT EXTENSION LH (for 4WD)

10. REMOVE FRONT BUMPER REINFORCEMENT EXTENSION RH (for 4WD)