GSIC - Global Service Information Center

# GENERATOR > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag activation.

2. REMOVE AIR CLEANER ASSEMBLY

1. Remove the clamp and disconnect the IAT connector.

1. Loosen the clamp of the turbocharger.

1. Slide the clamp and disconnect the ventilation hose.

1. Remove the 2 bolts and air cleaner.

3. REMOVE FAN AND GENERATOR V BELT

1. Using the pulley set bolt of the tensioner, rotate the tensioner pulley clockwise to loosen the belt's tension. Then remove the V belt.

4. REMOVE GENERATOR ASSEMBLY

1. Remove the nut and generator wire.

1. Disconnect the generator connector.

1. Remove the 2 bolts, adjusting bar and generator.