GSIC - Global Service Information Center

# REAR BUMPER (for Flat Type) > INSTALLATION

## for Preparation Click here

1. INSTALL REAR BUMPER ARM LH

1. Install the arm with the 2 bolts.

   Torque:
     45 N*m{ 459 kgf*cm , 33 ft.*lbf }

2. INSTALL REAR BUMPER ARM RH

1. Install the arm with the 2 bolts.

   Torque:
     45 N*m{ 459 kgf*cm , 33 ft.*lbf }

3. INSTALL REAR BUMPER BAR

1. Install the bumper with the 4 bolts.

   Torque:
     45 N*m{ 459 kgf*cm , 33 ft.*lbf }

1. Attach the 4 license plate light clamps.

1. Connect the 2 connector.

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.