GSIC - Global Service Information Center

# AIR FUEL RATIO SENSOR (for Sensor 1) > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE V-BANK COVER

1. Remove 2 nuts and cover.

3. REMOVE AIR FUEL RATIO SENSOR (for Bank 1 Sensor 1)

1. Disconnect the sensor connector.

1. Using SST, remove the sensor from the exhaust manifold.

   SST
     09224-00010

4. REMOVE AIR FUEL RATIO SENSOR (for Bank 2 Sensor 1)

1. Disconnect the sensor connector.

1. Using SST, remove the sensor from the exhaust manifold.

   SST
     09224-00010