GSIC - Global Service Information Center

### DTC P0607 Input Signal Circuit Malfunction

## for Preparation Click here

## DESCRIPTION

This DTC indicates the internal abnormalities of the ECM.

DTC No. | DTC Detection Condition | Trouble Area

P0607

When one of following conditions is met

1. Cruise control input signal is abnormal
2. Stop light switch input signal is abnormal

1. ECM

## INSPECTION PROCEDURE

1.CHECK FOR DTC

1. Delete the DTC.

1. Check for DTCs again.

   OK:
     No DTC is output.

| NG |

REPLACE ECM

OK |

END