GSIC - Global Service Information Center

# AIR CONDITIONING AND BLOWER UNIT > DISASSEMBLY

## for Preparation Click here

1. REMOVE NO. 3 AIR DUCT

1. Detach the 4 claws and remove the duct.

2. REMOVE AIR INLET DAMPER CONTROL CABLE SUB-ASSEMBLY

1. Detach the 3 claws and remove the cable.

3. REMOVE MODE CONTROL CABLE SUB-ASSEMBLY

1. Detach the 3 claws and remove the cable.

4. REMOVE BLOWER RESISTOR

1. Remove the 2 screws and blower resistor.

5. REMOVE BLOWER WITH FAN MOTOR SUB-ASSEMBLY

1. Remove the 3 screws and blower motor.