GSIC - Global Service Information Center

### FUEL SUPPLY PUMP > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE UNDER COVER (for 4WD)

3. REMOVE NO. 2 ENGINE UNDER COVER (for 4WD)

4. LOOSEN FUEL TANK CAP ASSEMBLY

5. DRAIN FUEL

6. DRAIN ENGINE COOLANT

7. DRAIN AUTOMATIC TRANSMISSION FLUID

8. REMOVE RADIATOR ASSEMBLY

9. REMOVE NO. 1 TIMING BELT COVER

10. REMOVE TIMING BELT

11. REMOVE FUEL SUPPLY PUMP