GSIC - Global Service Information Center

# 1GR-FE LUBRICATION > TORQUE SPECIFICATIONS

Part tightened | N*m | kgf*cm | ft.*lbf
Oil pump relief valve x Timing chain cover | 49 | 500 | 36
Oil pump cover x Timing chain cover | 9.0 | 92 | 80 in.*lbf
Oil pipe x Timing chain cover | 9.0 | 92 | 80 in.*lbf
Oil pressure switch x Oil filter bracket | 15 | 152 | 11
Oil pan drain plug x No. 2 oil pan | 40 | 408 | 30
Oil filter bracket x Timing chain cover | 19 | 194 | 14
Ignition coil x Cylinder head cover | 10 | 102 | 7
No. 1 oil pan x Cylinder block : for bolt A, B and nut | 21 | 214 | 15
No. 1 oil pan x Cylinder block | 9.0 | 92 | 80 in.*lbf
Oil strainer x No. 1 oil pan | 9.0 | 92 | 80 in.*lbf
No. 2 oil pan x No. 1 oil pan : for bolt | 9.0 | 92 | 80 in.*lbf
No. 2 oil pan x No. 1 oil pan : for nut | 10 | 102 | 7
V-bank cover x Cylinder head cover | 7.5 | 76 | 66 in.*lbf