GSIC - Global Service Information Center

### REAR AXLE SHAFT > REMOVAL

1. REMOVE REAR WHEEL

2. REMOVE BRAKE DRUM

3. REMOVE REAR SPEED SENSOR LH (w/ ABS)

4. REMOVE REAR BRAKE SHOE (for 2WD)

5. REMOVE REAR BRAKE SHOE (for 4WD)

6. DISCONNECT BRAKE LINE AND PARKING BRAKE CABLE

7. REMOVE REAR AXLE SHAFT WITH BACKING PLATE

8. REMOVE O-RING FROM REAR AXLE HOUSING

9. REMOVE REAR AXLE SHAFT OIL SEAL

10. REMOVE REAR AXLE BEARING INNER RETAINER AND (W/ ABS) ABS SPEED SENSOR ROTOR

11. REMOVE REAR AXLE SHAFT

12. REMOVE REAR AXLE HUB BOLT

13. INSPECT REAR AXLE SHAFT LH

14. REMOVE REAR AXLE SHAFT OUTER OIL SEAL

15. REMOVE REAR AXLE SHAFT BEARING