GSIC - Global Service Information Center

# CENTER AIRBAG SENSOR ASSEMBLY > REMOVAL

## for Preparation Click here

CAUTION:

  Be sure to read the precautionary notices concerning the SRS airbag system before servicing (Click here).

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE SHIFT LEVER KNOB SUB-ASSEMBLY (M/T)

3. REMOVE TRANSFER SHIFT LEVER KNOB SUB-ASSEMBLY (4WD)

4. REMOVE CONSOLE PANEL SUB-ASSEMBLY UPPER

NOTICE:

  Be careful not to damage the instrument panel lower and console box with the claws of the console panel upper.

1. Detach the 12 claws and remove the console panel.

5. REMOVE CONSOLE BOX ASSEMBLY

1. Remove the 4 screws <F> and 2 bolts <E>.

1. Using a clip remover, remove the 2 clips and console box.

6. REMOVE CENTER AIRBAG SENSOR ASSEMBLY

1. Disconnect the sensor connector.

1. Remove the 3 bolts and sensor.