GSIC - Global Service Information Center

# ENGINE COOLANT TEMPERATURE SENSOR > INSPECTION

## for Preparation Click here

1. INSPECT ENGINE COOLANT TEMPERATURE SENSOR

1. Measure the resistance between the terminals.

   Standard resistance:

     Condition | Specified Condition
     Approx. 20°C (68°F) | 2.32 to 2.59 Ω
     Approx. 80°C (176°F) | 0.310 to 0.326 kΩ

   1. If the result is not as specified, replace the sensor.

   NOTICE:
     When checking the ECT sensor in the water, keep the terminals dry. After the check, wipe the sensor dry.