GSIC - Global Service Information Center

# 1KD-FTV ENGINE MECHANICAL > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Engine mounting bracket RH x Cylinder block | 68 | 694 | 50
Engine mounting bracket LH x Cylinder block | 68 | 694 | 50
Engine coolant temperature sensor x Cylinder head | 20 | 204 | 15
Camshaft position sensor x Timing gear case | 8.5 | 87 | 75 in.*lbf
Crankshaft position sensor x Timing gear case | 8.5 | 87 | 75 in.*lbf
Vane pump x Timing gear case | 39 | 398 | 29
Vacuum pump x Timing gear case cover | 21 | 214 | 16
Intake manifold x Cylinder head | 29 | 296 | 21
Oil level gage guide x Intake manifold | 8.0 | 82 | 71 in.*lbf
Diesel throttle body bracket x Intake air connector | 20 | 204 | 15
Diesel throttle body bracket x Intake manifold | 20 | 204 | 15
Diesel throttle body assembly x Intake air connector | 20 | 204 | 15
Vacuum switching valve bracket x Intake air connector | 20 | 204 | 15
Vacuum switching valve bracket x Intake manifold | 20 | 204 | 15
Manifold stay x Intake manifold | 19 | 194 | 14
Manifold stay x Cylinder block | 19 | 194 | 14
Water inlet x Cylinder head | 19 | 194 | 14
Compressor mounting bracket No. 1 x Cylinder block | 47 | 479 | 35
V-ribbed belt tensioner assembly x Cylinder block | 21 | 214 | 16
V-ribbed belt tensioner assembly x Water pump assembly | 21 | 214 | 16
Generator bracket x Timing gear case cover | 25 | 255 | 18
Generator bracket x Generator assembly | 25 | 255 | 18
Exhaust manifold x Cylinder head | 40 | 408 | 30
Crankshaft pulley x Crankshaft | 365 | 3,722 | 270
Timing belt No. 1 cover x Timing belt No. 2 cover | 6.0 | 61 | 53 in.*lbf
Air cleaner pipe sub-assembly No. 2 x Cylinder head | 20 | 204 | 15
Engine cover bracket x Cylinder head | 18 | 184 | 13
Engine mounting bracket RH x Body | 38 | 388 | 28
Engine mounting bracket LH x Body | 38 | 388 | 28
Rear end plate x Cylinder block | 8.0 | 82 | 71 in.*lbf
Cooler compressor assembly x Compressor mounting bracket No. 1 | 50 | 510 | 37
Pressure feed tube x Vane pump | 51 | 520 | 38
Ground cable x Body | 30 | 306 | 22
Engine room J/B wire x Engine room J/B | 13 | 133 | 22
Air cleaner assembly x Body | 14 | 143 | 10
Hood sub-assembly x Hood hinge | 11.5 | 117 | 8.4
Timing belt idler pulley x Cylinder block | 35 | 350 | 25
Timing belt tensioner x Cylinder block | 13 | 133 | 10
Timing belt No. 2 cover x Cylinder head | 10 | 102 | 7
Timing belt No. 2 cover x Cylinder block | 10 | 102 | 7
Water hose clamp x Cylinder head | 18 | 184 | 13
Bearing cap x Cylinder head | 19 | 194 | 14
Camshaft timing pulley x Camshaft | 98 | 1,000 | 72
Cylinder head cover x Cylinder head | 9.0 | 92 | 80 in.*lbf
Cylinder head sub-assembly x Cylinder block | 1st | 85 | 867 | 63
2nd | Turn 90° | Turn 90° | Turn 90°
3rd | Turn 90° | Turn 90° | Turn 90°
Engine rear oil seal retainer x Cylinder block | Bolt A | 13 | 133 | 9.6
Bolt B | 16 | 163 | 12
Supply pump x Timing gear case | 1 | 214 | 15
Injection gear x Supply pump | 64 | 652 | 47
Engine rear oil seal retainer x Cylinder block | 13 | 133 | 10
Timing gear case x Cylinder block | Bolt | 13 | 133 | 10
Union bolt | 16 | 163 | 12
Oil strainer x Cylinder block | 8.0 | 82 | 71 in.*lbf
Oil pan x Cylinder block | 16 | 163 | 12
Oil pan x Timing gear case | 16 | 163 | 12
Engine oil level sensor x Oil pan | 8.0 | 82 | 71 in.*lbf
Driven gear No. 1 x No. 1 balance shaft sub-assembly | 36 | 367 | 27
Driven gear No. 2 x No. 2 balance shaft sub-assembly | 36 | 367 | 27
Thrust washer x Cylinder block | 13 | 133 | 10
Idle gear thrust plate x Idle gear shaft No. 1 | 50 | 510 | 37
Water pump assembly x Cylinder block | 13 | 133 | 10
Camshaft timing pulley x Camshaft | 98 | 1,000 | 72
Timing belt No. 2 cover x Cylinder head, Cylinder block | 10 | 102 | 7
Nozzle holder clamp x Cylinder head | 22 | 220 | 16
Nozzle leakage pipe x Injector | Hollow screw | 16 | 163 | 12
Union bolt | 13 | 133 | 10
Camshaft bearing cap x Cylinder head | 19 | 194 | 14
Cylinder head cover x Cylinder head | 9.0 | 92 | 80 in.*lbf
Cylinder head x Cylinder block | 1st | 85 | 867 | 63
2nd | Turn 90° | Turn 90° | Turn 90°
3rd | Turn 90° | Turn 90° | Turn 90°
Timing gear cover x Timing gear case | 13 | 133 | 10
Common rail assembly x Cylinder block | 38 | 387 | 28
Nozzle leakage pipe No. 2 x Cylinder head | 21 | 214 | 16
Connecting rod cap x Connecting rod | 1st | 35 | 357 | 26
2nd | Turn 90° | Turn 90° | Turn 90°
Oil check valve sub-assembly x Cylinder block | 26 | 265 | 19
Crankshaft bearing cap x Cylinder block | 1st | 50 | 510 | 37
2nd | Turn 90° | Turn 90° | Turn 90°
Straight screw plug No. 1 x Cylinder block | 20 | 204 | 15