GSIC - Global Service Information Center

# 1KD-FTV LUBRICATION > SERVICE DATA

Oil pressure | at idle speed | 29 kPa (0.3 kgf/cm2, 4.2 psi) or more
at 3,000 rpm | 160 to 490 kPa (1.6 to 5.0 kgf/cm2, 23 to 71 psi)
Supply pump drive shaft pulley | Thrust clearance | 0.15 to 0.55 mm (0.0059 to 0.0217 in.)
Oil pump | Tip clearance | Standard | .0.060 to 0.160 mm (0.0024 to 0.0063 in.)
Maximum | 0.21 mm (0.0083 in.)
Body clearance | Standard | 0.100 to 0.170 mm (0.0039 to 0.0066 in.)
Maximum | 0.20 mm (0.0079 in.)
Side clearance | Standard | 0.030 to 0.090 mm (0.0012to 0.0036 in.)
Maximum | 0.15 mm (0.0059 in.)