GSIC - Global Service Information Center

# REAR SEAT ASSEMBLY (for Double Cab) > REMOVAL

## for Preparation Click here

1. REMOVE REAR SEAT HINGE COVER LH

1. Using a screwdriver, detach the 2 claws labeled A.

   HINT:
     Tape the screwdriver tip before use.

1. Pull the hinge cover in the direction indicated by the arrow in the illustration to detach the claw labeled B. Then remove the hinge cover.

2. REMOVE REAR SEAT HINGE COVER RH

HINT:

  Use the same procedures described for the LH side.

3. REMOVE REAR SEAT ASSEMBLY

1. Remove the fold seat stopper band from the knob and fully extend the band.
   Pull the fold seat stopper band and fold up the seat as shown in the illustration.

1. Pull the inner belts out from between the seat cushion and seatback.

1. Remove the 4 bolts.

1. Lift up the seat in the direction indicated by the arrow in the illustration to detach the 2 hooks from the vehicle body. Then remove the seat.

   NOTICE:
     Be careful not to damage the vehicle body.