GSIC - Global Service Information Center

# CAMSHAFT TIMING OIL CONTROL VALVE ASSEMBLY > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE V-BANK COVER

1. Remove the 2 nuts and the V-bank cover.

3. REMOVE NO. 2 VENTILATION HOSE

4. REMOVE AIR CLEANER ASSEMBLY

1. Disconnect the vacuum hose.

1. Disconnect the MAF meter connector.

1. Remove the 2 wire harness clamps.

1. Loosen the 2 hose clamps.

1. Remove the 2 bolts and air cleaner.

5. REMOVE THROTTLE BODY

1. Disconnect the throttle motor connector.

1. Remove the 4 bolts and throttle body.

1. Remove the gasket from the intake air surge tank.

6. REMOVE CAMSHAFT TIMING OIL CONTROL VALVE (for Bank 1)

1. Disconnect the oil control valve connector.

1. Remove the bolt and oil control valve.

1. Remove the O-ring from the oil control valve.

7. REMOVE CAMSHAFT TIMING OIL CONTROL VALVE (for Bank 2)

1. Disconnect the oil control valve connector.

1. Remove the bolt and oil control valve.

1. Remove the O-ring from the oil control valve.