GSIC - Global Service Information Center

# SPEEDOMETER DRIVEN GEAR > INSTALLATION

## for Preparation Click here

1. INSTALL SPEEDOMETER DRIVEN GEAR SUB-ASSEMBLY

1. Install a new O-ring to the driven gear.

1. Install the driven gear to the sensor with the clip.

2. INSTALL VEHICLE SPEED SENSOR WITH SPEEDOMETER DRIVEN GEAR SUB-ASSEMBLY

1. Install the sensor with the driven gear with the bolt.

   Torque:
     11.5 N*m{ 117 kgf*cm , 8 ft.*lbf }

1. Connect the sensor connector.

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.