GSIC - Global Service Information Center

# 1GR-FE COOLING > SERVICE DATA

Water inlet housing with thermostat:

  Condition | Specified Condition
  Valve opening temperature | 80 to 84°C (176 to 183°F)
  Valve lift | 8.0 mm (0.31 in.) or more at 95°C 203°F)

Radiator cap:

  Item | Specified Condition
  Standard value (for brand-new cap) | 93.3 to 122.7 kPa (0.95 to 1.25 kgf*cm2, 13.5 to 17.8 psi)
  Minimum standard value (after using cap) | 78.5 kPa (0.8 kgf*cm2, 11.4 psi)