GSIC - Global Service Information Center

### DTC P0985 Shift Solenoid "E" Control Circuit Low (Shift Solenoid Valve SR)

### DTC P0986 Shift Solenoid "E" Control Circuit High (Shift Solenoid Valve SR)

## for Preparation Click here

## DESCRIPTION

Shifting from 1st to 5th is performed in combination with the ON and OFF operation of the shift solenoid valves SL1, SL2, S1, S2 and SR, which is controlled by the ECM. If an open or short circuit occurs in the shift solenoid valves, the ECM controls the remaining normal shift solenoid valve to allow the vehicle to be operated safely (Click here).

DTC No. | DTC Detection Condition | Trouble Area

P0985

ECM detects short in solenoid valve SR circuit 2 times when solenoid valve SR is operated (1 trip detection logic)

1. Short in shift solenoid valve SR circuit
2. Shift solenoid valve SR
3. ECM

P0986

ECM detects open in solenoid valve SR circuit 2 times when solenoid valve SR is not operated (1 trip detection logic)

1. Open in shift solenoid valve SR circuit
2. Shift solenoid valve SR
3. ECM

## MONITOR DESCRIPTION

These DTCs indicate an open or short in the shift solenoid valve SR circuit. When there is an open or short circuit in any shift solenoid valve circuit, the ECM detects the problem and illuminates the MIL and stores the DTC. When the shift solenoid valve SR is ON, if resistance is 8 Ω or less, the ECM determines that there is a short in the shift solenoid valve SR circuit.
When the shift solenoid valve SR is OFF, if resistance is 100 kΩ or more, the ECM determines that there is an open in the shift solenoid valve SR circuit (Click here).

## WIRING DIAGRAM

## INSPECTION PROCEDURE

HINT:

  The shift solenoid valve SR turns ON/OFF normally when the shift lever is on D:

ECM gear shift command | 1st | 2nd | 3rd | 4th | 5th
Shift solenoid valve SR | OFF | OFF | OFF | OFF | ON

1.INSPECT TRANSMISSION WIRE (SHIFT SOLENOID VALVE SR)

1. Disconnect the E1 wire connector.

1. Measure the resistance of the wire connector.

   Standard resistance:

     Tester Connection | Condition | Specified Condition
     7 - Body ground | 20°C (68°F) | 11 to 15 Ω

| NG |

Go to step 3

OK |

2.CHECK WIRE HARNESS (TRANSMISSION WIRE - ECM)

1. Disconnect the E16 ECM connector.

1. Measure the resistance of the wire harness side connector.

   Standard resistance:

     Tester Connection | Condition | Specified Condition
     E16-9 (SR) - Body ground | 20°C (68°F) | 11 to 15 Ω

| NG |

REPAIR OR REPLACE HARNESS AND CONNECTOR

OK |

REPLACE ECM

3.INSPECT SHIFT SOLENOID VALVE SR

1. Remove the shift solenoid valve SR.

1. Measure the resistance of the solenoid valve.

   Standard resistance:
     5.0 to 5.6 Ωat 20°C (68°F)

1. Connect the battery's positive (+) lead to the terminal of the solenoid connector, and the negative (-) lead to the solenoid body.

   OK:
     Solenoid makes operating noise.

| NG |

REPLACE SHIFT SOLENOID VALVE SR

OK |

REPAIR OR REPLACE TRANSMISSION WIRE